OpenStudio Version 1.9.0

Release Notes – 9/25/2015

These release notes describe version 1.9.0 of the OpenStudio software suite developed by the National Renewable Energy Laboratory (NREL), Buildings and Thermal Systems, Commercial Buildings Research Group, Tools Development Section, and associated collaborators. The notes are organized into the following sections:

* Where to Find OpenStudio Documentation
* Installation Notes
* Overview

# Where to Find OpenStudio Documentation

* OpenStudio release documentation, including these release notes, tutorials, and other user documentation, is available at <https://www.openstudio.net/>.
* C++ API documentation is available at <https://openstudio-sdk-documentation.s3.amazonaws.com/index.html>.
* Measure development documentation is available at <http://nrel.github.io/OpenStudio-user-documentation/reference/measure_writing_guide/>.

# Installation Notes

OpenStudio is supported on Windows 7 – 8.1, OS X 10.9 – 10.10, and 64-bit Ubuntu 14.04.

OpenStudio 1.8.0 supports EnergyPlus Release 8.3.0, which is bundled with the OpenStudio installer. It is no longer necessary to download and install EnergyPlus separately. However, an installer is available at <https://github.com/NREL/EnergyPlus/releases/tag/v8.3.0>. Other builds of EnergyPlus 8.3 are not supported by OpenStudio 1.8.0.

Say something about Radiance bundling here…

## Installation Steps

* The OpenStudio SketchUp Plug-in requires [SketchUp 2015](http://www.sketchup.com/) (not available for Linux). The OpenStudio SketchUp Plug-in does not support older versions of SketchUp. SketchUp 2015 is available in 32 and 64-bit versions; the 32-bit version of OpenStudio on Windows will only work with the 32-bit version of SketchUp 2015, and the 64-bit version of OpenStudio will only work with the 64-bit version of SketchUp 2015.
* Download and install [OpenStudio](https://www.openstudio.net/downloads).
* Setup a Building Component Library (BCL) account to access online building components and measures. [View instructions on how to setup your account and configure the key in OpenStudio](http://nrel.github.io/OpenStudio-user-documentation/getting_started/getting_started/).

## Optional Installation Steps

* For Radiance integration, download and install [Radiance](http://nrel.github.io/OpenStudio-user-documentation/getting_started/getting_started/).

# Overview

OpenStudio 1.9.0 adds a substantial number of new HVAC features. Among the new features are three entirely new categories of HVAC capability beyond the routine component additions. The first new category is a family of availability mangers that allow for detailed control over the air system period of operation. With these new availability manager control inputs, it is possible to have detailed control over night cycling, night ventilation, optimum morning start, temperature based on/off and more. The second new category of HVAC capability included in this release is another family of control related inputs known as plant operation schemes. With plant operation schemes it is possible to control the sequencing of plant system supply components relative to one another and also considering ambient conditions. Finally, in a third new category, OpenStudio has added support for dual duct air based systems. At this point these new features are available through the OpenStudio API and Measures, however support for the user interface will be added in a future release. All of these features are backwards compatible, meaning users now have access to detailed control inputs, but the established OpenStudio default control remains in place, meaning these new features can be utilized on an as needed basis and existing models will continue to operate in the same way. Examples and tutorials of applying these new features will be available in the weeks following the release of OpenStudio 1.9.0.

There are significant additions at the HVAC component level too, meaning there is a large number of new coil types, Zone HVAC, and plant components. Of particular interest are a number of new variable speed DX coils, new zone mixing inputs, a new Zone HVAC model that accommodates natural ventilation, and idealized plant components that allow a user defined constant temperature source on the supply side, and a user defined load on the demand. The full list of new input object types is included below. All of these are available in the OpenStudio API and Measures, and many of them are available in the graphical interface through drag and drop.

ZoneCrossMixing • ZoneMixing • SolarCollectorPerformanceFlatPlate • SolarCollectorFlatPlateWater • SolarCollectorIntegralCollectorStorage • SolarCollectorPerformanceIntegralCollectorStorage • SolarCollectorFlatPlatePhotovoltaicThermal • ZoneVentilationDesignFlowRate • FluidCoolerTwoSpeed • FluidCoolerSingleSpeed • PipeOutdoor • PipeIndoor • Duct• AvailabilityManagerHybridVentilation • CoilSystemCoolingWaterHeatExchangerAssisted • CoilSystemCoolingDXHeatExchangerAssisted • PlantEquipmentOperationOutdoorDewpoint • PlantEquipmentOperationOutdoorWetBulb • TemperingValve • ChillerAbsorption • ChillerAbsorptionIndirect • CoilCoolingDXTwoStageWithHumidityControlMode • AirTerminalDualDuctVAV • AvailabilityManagerOptimumStart • AvailabilityManagerDifferentialThermostat • ThermalStorageIceDetailed • GroundHeatExchangerHorizontalTrench • PlantEquipmentOperationOutdoorRelativeHumidity • AvailabilityManagerNightVentilation • PlantEquipmentOperationOutdoorDryBulbDifference • PlantEquipmentOperationOutdoorDewpointDifference • PlantEquipmentOperationOutdoorWetBulbDifference • PlantEquipmentOperationOutdoorDryBulb • HeaderedPumpsConstantSpeed • HeaderedPumpsVariableSpeed • WaterHeaterHeatPump • CoilPerformanceDXCooling • CoilWaterHeatingAirToWaterHeatPump • CoilHeatingWaterToAirHeatPumpVariableSpeedEquationFit • CoilHeatingDXVariableSpeed • CoilCoolingWaterToAirHeatPumpVariableSpeedEquationFit • SetpointManagerSingleZoneHumidityMaximum • ThermalStorageChilledWaterStratified • SetpointManagerColdest • EvaporativeFluidCoolerTwoSpeed • SetpointManagerMultiZoneCoolingAverage • SetpointManagerMultiZoneHeatingAverage • ZoneHVACDehumidifierDX • ZoneHVACEnergyRecoveryVentilatorController • ZoneHVACEnergyRecoveryVentilator • CoilCoolingDXVariableSpeed • CentralHeatPumpSystem • SetpointManagerMultiZoneHumidityMaximum • CoilHeatingDXMultiSpeed • SetpointManagerFollowSystemNodeTemperature • SetpointManagerSingleZoneOneStageCooling • SetpointManagerSingleZoneOneStageHeating • SetpointManagerMultiZoneMaximumHumidityAverage • SetpointManagerMultiZoneMinimumHumidityAverage • SetpointManagerReturnAirBypassFlow • SetpointManagerFollowGroundTemperature • ChillerHeaterPerformanceElectricEIR • PlantComponentTemperatureSource • ZoneHVACUnitVentilator • WaterHeaterStratified • ZoneHVACBaseboardRadiantConvectiveWater • ZoneHVACBaseboardRadiantConvectiveElectric • LoadProfilePlant

## OpenStudio 1.9.0 includes several other minor features as well as many bug fixes. For a full list of changes included in OpenStudio 1.9.0, please see the [complete changelog](https://github.com/NREL/OpenStudio/blob/v1.8.0/CHANGELOG.md).

## Issue Statistics Since Previous Release

* 108 new issues were filed since the 1.7.0 release of OpenStudio (not including opened pull requests).
* 53 issues were closed since the 1.7.0 release of OpenStudio (not including closed pull requests).